Categories:Navigation
License:MIT
Web Site:
Source Code:https://github.com/illarionov/RtkGps
Issue Tracker:https://github.com/illarionov/RtkGps/issues

Auto Name:RtkGps
Summary:RTKLIB rtknavi port
Description:
Real-time standard and precise GNSS Positioning on Android using an external
Bluetooth or USB GPS receiver; based on RTKLIB.

* GPS, GLONASS, Galileo, QZSS, BeiDou and SBAS Navigation systems
* Single, DGPS/DGNSS, Kinematic, Static, Moving-Baseline, Fixed, PPP-Kinematic, PPP-Static and PPP-Fixed positioning modes.
* RINEX 2.10,2.11,2.12 OBS/NAV/GNAV/HNAV/LNAV/QNAV, RINEX 3.00,3.01,3.02 OBS/NAV,RINEX 3.02 CLK,RTCM ver.2.3,RTCM ver.3.1 (with amendment 1-5), RTCM ver.3.2, BINEX, NTRIP 1.0, NMEA 0183, SP3-c, ANTEX 1.4, IONEX 1.0, NGS PCV and EMS 2.0.
* Proprietary protocotols: NovAtel: OEM4/V/6,OEM3,OEMStar,Superstar II, Hemisphere: Eclipse,Crescent, u-blox: LEA-4T/5T/6T, SkyTraq: S1315F, JAVAD GRIL/GREIS, Furuno GW-10-II/III and NVS NV08C BINR, TCP/IP, NTRIP, local log file
* Bluetooth and USB OTG communication
* experimental SiRF IV protocol support

Status: Alpha
.

Repo Type:git
Repo:https://github.com/illarionov/RtkGps.git

Build:1.0,1
    commit=1b27b7
    init=sed -i 's/@/:\/\//g;s/:little/\/little/g;s/:illar/\/illar/g' .gitmodules && \
        git submodule update --init
    forceversion=yes
    scanignore=jni/simonlynen_android_libs/lapack/jni/clapack/INSTALL
    buildjni=yes

Maintainer Notes:
The scanner is tripped by binaries that are only used for testing; see the README.install.
Could rm test* rather than scanignore but fdroid doesn't recover afterwards,
since they're submodules
.

Auto Update Mode:None
Update Check Mode:RepoManifest
Current Version:1.0
Current Version Code:1
